LITERATURE REVIEW

December 13, 2019

Mary McGuinn, mem563@cornell.edu

INTRODUCTION

The upflow anerobic sludge blanket (UASB) is a single tank reactor that treats wastewater. The general process is completed by having sludge enter the reactor from the bottom. Light and dispersed particles are washed out of the process, while heavier particles collect and retain within the system. These heavier particles then form flocs consisting of inorganic and organic matter (Hulshoff Pol et al. 2003). After a start-up period, a dense sludge blanket consisting of flocs develops creating an environment for biological reactions to take place. As flow passes upward through the sludge blanket, the soluble organic compounds in the influent convert to biogas.

The UASB reactor is an increasingly common method of wastewater treatment because it has a high reduction of biochemical oxygen demand (BOD), low sludge production, high organic and hydraulic loading rate tolerance, and biogas production (UASB|SSWM). However, although the UASB reactor can handle high organic and hydraulic loading rates, if variable, treatment may also be unstable. Furthermore, most UASB reactors require a constant source or electricity. The effluent and sludge from the reactor require further treatment and appropriate discharge (UASB|SSWM).

This literature review will focus on the review by Chong et al. (2012) and complementing research papers. It will discuss UASB start-up, post-treatment options, and use of resulting biogas.

START-UP

Before direct treatment of wastewater, the UASB reactor needs a start-up period using selected nutrients as substrate. This start-up is a strong determinant of the effectiveness and stability of the reactor, determined by many physical, chemical, and biological parameters (Ghangrekar et al., 1996). Municipal wastewater takes two-eight months on average to achieve full efficiency (Chong et al., 2012, Lettinga et al., 1993, Vlyssides et al., 2008). To shorten this period, the standard procedure is to inoculate the reactor with active microorganisms or granules (Bhatti 2014).

This procedure to develop granules can be split into four steps (Schmidt 1996, Escudie et al. 2011):

1. Transport of cells to a substratum
2. Initial reversible adsorption to the substratum by physicochemical forces
3. Irreversible adhesion of cells to the substratum by microbial appendages and/or polymer
4. Multiplication of the cells and development of granules

Ghangrekar et al. (1996) observed that COD removal efficiency is greatly influenced by start-up and sludge loading rates (SLR). For example, a reactor which started with 0.6 kg COD/kg VSS/d resulted in ~50% COD removal at steady state, and it did not improve through operation time. However, a reactor which started with 0-0.3 kg COD/kg VSS/d resulted in a better performance with more than 90% COD removal at steady state. This study also suggests that organic loading rates and SLR are determiners in how much time is required for a reactor to reach steady state.

Furthermore, other additives can be incorporated to increase the start-up time. See Table 3 in the Appendix for the results of recent studies on theses additives.

POST-TREATMENT

A UASB reactor has an inability to meet all disposal standards for degraded soluble matter, colloidal, nutrients, and pathogens. Therefore, in order to meet present standards, a secondary treatment, also known as post-treatment or polishing process, is required (Khan 2011).

**Options**

There are seven common post-treatment options for the UASB reactor. See Table 1 for a summary of the advantages and disadvantages of the options below.

1. *Activated Sludge (AS)*

AS uses microorganisms to feed on organic components in the wastewater to improve effluent. In general, the microorganisms grow to form floc (particles which bind together) from the organic material and suspended solids. The floc settles which allows the high-quality effluent to separate (‘Explaining the Activated Sludge Process’).

1. *Sequencing-batch Reactor (SBR)*

SBR uses two or more batch reactors to optimize the performance of the system. However, in most SBR single processors, equalization, primary and secondary clarification, and biological treatment can be accomplished with a single reactor. A common process for a post-treatment with an SBR is such that wastewater enters a partially filled reactor with biomass acclimated to the wastewater constituents. Once full, the system works as the AS system but without continuous influent or effluent flow. Excess biomass is wasted throughout the process (EPA SBR).

1. *Trickling Filter (TF),* or biofilter (BF)

TFis an attached-growth process system. Meaning, it is an aerobic treatment system that incorporates microorganisms attached to a medium to remove organic matter from the wastewater (EPA TF). As water travels through the filter, organics are degraded by the biofilm covering the filter (SSWM).

1. *Downflow Hanging Sponge (DHS)*

DHS uses simple and economic PUR foams (packing material). This method is used to decrease energy demand, maintenance, and operating costs. This post-treatment option achieves a near perfect BOD removal and high coliforms removal (Chong et al. 2012).

1. *Stabilizing Pond (SP)*

SP is used to recover nutrients from the UASB effluents. It is a man-made body of water which can be used individually or as a series for treatment. The types of SPs are 1) anaerobic ponds commonly used to reduce the organic load, 2) facultative ponds to remove BOD, and 3) aerobic ponds to remove pathogens and contaminants. It is recommended that SPs be used in this respective series (SSWM).

1. *Rotating-biological Contactor (RBC)*

Like the TF, RBC is a fixed-bed reactor. However, the RBC consists of foam disks (polystyrene or polyurethane) mounted to a steel shaft and partially submerged in the effluent solution. These disks rotate and allow wastewater to flow through. RBCs allow for aeration and degradation of dissolved organic pollutants and nutrients.

1. *Constructed Wetland (CW)*

CW is an artificial wetland which serves as a biofilter. This allows for natural processes to degrade organic matter and remove nutrients, pathogens, sediments, and pollutants from the wastewater. A CW is either, or a combination of, subsurface flow and free-water-surface flow less than one meter deep planted with vegetation. It aides in microorganism growth and degradation of organic matter (Chong et al. 2012).

Other post-treatment options which will not be discussed include dissolved-air-flotation, cascade-sponge reactor, and membrane reactors.

*Table 1: Summary of Post-treatment Advantages and Disadvantages (Chong et al. 2012)*

|  |  |  |
| --- | --- | --- |
| **Option** | **Advantages** | **Disadvantages** |
| *Activated Sludge* | * High efficiency * Resistant to variable flow and toxic loads * Consistent nutrification | * High mechanization level * High construction costs * Requires energy * Noise and aerosol pollution |
| *Sequencing-batch Reactor* (EPA SBR) | * Flexible operation and control * Low cost with limited clarifiers | * Sophisticated maintenance requirements * High maintenance cost * Potential plugging of aeration devices and equalization requirement |
| *Trickling Filter*  (EPA TR) | * Simple and reliable * Small land requirement * Efficient in nitrification | * Moderate technical experience required for management * Accumulation of excess biomass * Regular operation requirements * Vector and odor issues |
| *Downflow Hanging Sponge* | * Low cost * Simple maintenance * Simultaneous nitrification and denitrification * No external aeration input | * Need of proper influent-distribution system design for full-scale plants and first generation * Less favorable for shock loads and nitrogen removal |
| *Stabilizing Pond* | * Low maintenance requirements * No energy requirement * Sludge accumulates slowly * High suspended solids (SS) production | * Large land requirement * Recovery of nutrients and removal of fecal coliforms affected by temperatures |
| *Rotating-biological Contactor* | * Low energy requirement * Resistance to high organic loadings * Low energy requirement * Easy maintenance | * Excess sludge removal unknown * More units of higher HRT’s required for treatment at low temperatures |
| *Constructed Wetland* | * Easy construction and maintenance * Low surplus sludge | * High land requirement * Gravel clogs (e.g. near the inlet, shortening the lifespan of the wetland) * Limited nutrient and pathogen removal |

\*See Tables 4-5 in the Appendix for a more detailed advantages and disadvantages list from Chong et al. (2012).

**Integrated Systems**

Below are effluent results of the aforementioned post-treatment options coupled with a UASB reactor. This list is not all inclusive. See Chong et al. (2012) for full results.

*Table 2: Treatment Performance of Integrated UASB and Post-treatment Systems* (adap. Chong et al. 2012)

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | **T (oC)** | **UASB** | | | | | **Post-treatment** | | | | **Concentration in final effluent (mg/L)**  **[Average removal efficiency (%)]** | | | | |
| **System Combination** |  | **Size** | **HRT (h)** | **OLR**  **(kg COD/ m3/d)** | **COD Inf. (mg/L)** | **COD Eff. (mg/L)** | **Size** | **HRT (h)** | **Other** | **COD** | | **BOD** | **TSS** | **NH4-N** |
| *UASB + AS* | 30 | 0.416 | 4 | 2.3-4.4 | 558 | 115 | 0.023 | 2.8 | **F/M**  0.6-0.9 | 55 [90] | |  | 15 [91] |  |
| 15-30 | 0.396 | 3.2 | 2.6 | 341 | 225 | 0.3 | 2.5 | 1.2 | 46 [87] | |  | 8 [92] |  |
| *UASB + SBR* | 21 | 150 L | 6 | 2.1 | 569 | 228 | 90 L |  | **Aeration (h)**  22  10  4  2 | 46 [92]  46 [92]  46 [92]  51 [91] | |  | 16 [88]  18 [86]  21 [84]  21 [84] | 0 [100]  0 [100]  0.5 [98]  33 [69] |
| *UASB + TF* | Sub- tropical | 0.416 | 4 | 3.8 | 521 | 148 | 0.06 | 3  1.5  0.8 |  | 80 [86]  72 [83]  113 [78] | | 32 [90]  23 [92]  55 [81] | 11 [91]  21 [83]  33 [73] |  |
| 26 | 0.416 | 5.6 | 1.9 | 437 | 108 | 0.106 | 1.5 |  | 82 [81] | | 27 [87] | 17 [89] |  |
| *UASB + DHS*  *(1st generation)* | 25 | 0.155 | 7 | 2.3 | 672 | 144 | 1.215 L | 1.3 | parallels | 42 [94] | | 2 [99] | 0 [100] | 7 [75] |
| *UASB + DHS*  *(2nd generation)* | 25 | 0.155 | 6 | 1.57 | 393 | 165 | 51 L | 2 | parallels  series | 65 [84]  68 [81] | | 4 [97]  10 [94] | 28 [79]  46 [63] | 20 [52]  15 [61] |
| 6 | 1.57 | 393 | 165 | 51 L | 2 | parallels  series | 65 [84]  65 [83] | | 8 [95]  4 [97] | 28 [79] | 12 [70]  20 [50] |
| *UASB + SP*  *(Averages)* |  | 0.04-4477 | 0.3-9.8 |  | 318-871 | 151-337 | 1.44-49333 | 1.1-15 d | **Depth (m)**  0.4-2 | 110 [73] | | 33 [85] | 60 [77] | 7.6 [64] |
| *UASB + RBC*  *(Averages)* | 12-21 | Single RBC with polystyrene foam disks | | | | | | 2.5-5 | **SLR (g COD/m2/d)**  10.5-20 | 79 [85] | | **TKN**  39 [35] | **EC**  3.4E5 [1.5] | 32 [32] |
| Single RBD with polyurethane rotating disks | | | | | | 2.5-5 | **SLR (g COD/m2/d)**  4-11 | 68 [87] | |  | 2.4E4 [2.4] | 6 [88] |
| Series RBS (2-3x) | | | | | | 2.5-10 | **SLR (g COD/m2/d)**  6.5-47.25 | 56 [89] | | 8 [86] | 8.2E4 [2.6] | 13 [75] |
| *UASB + CW*  *(Averages)* | 14-38 | 1.3-25.5 | 6-11 | 0.7-2.2 | 315-1050 | 117-525 | 0.8-78 | 1.2-10.8 d | **SLR (g COD/m2/d)**  7.2-52.8 | 47 [82] | | 17 [89] | 12 [89] | 17 [38] |

\*For a relative comparison, see Table 6 in the Appendix, outlined by Chong et al. (2012).


BIOGAS

Biogas is a clean, renewable source of energy that is produced from the decomposition of organic waste in an anaerobic environment, such as the UASB reactor. A gas is released that is a mixture of 50-70% methane, 30-40% carbon dioxide (Tanigawa 2017), and other gases. This raw biogas can be used for fuel, electricity, and heat. Furthermore, biogas is a reliable energy feedback which is healthier for the user over other energy sources, such as biomass.

*Renewable natural gas (RNG)* is biomethane, treated biogas so it retains no carbon dioxide, water vapor, or other contaminating gases. RNG is used as a replacement of natural gas and is used more frequently than raw biogas for energy.

See Figure 1 for the process to create biogas and RNG.

*Figure 1: Biogas Process (Tanigawa 2017)*



As shown in figure 1, biogas can not only provide heat and electricity as a fuel, but also the digestate from the collection process creates a slurry which can be used as fertilizer.

**Use of Raw Biogas**

Raw biogas can be used directly from the UASB reactor, however for that to occur, the method of use, e.g. a stove burner, needs to be directly connected to the system itself through a hose or pipe. Furthermore, when biogas is used in its raw form, it is much less efficient than if it were converted into RNG. Therefore, the appliance which uses the fuel most be adapted to maximize the energy potential coming from the raw biogas.

*Household Burner:* Using biogas with a stovetop is a great example of how to convert the appliance to use raw biogas. In order to alter a stove top to maximize its performance and increase flow of gas, it is recommended (without study) that the cross-section of the injector be expanded 2-4 times than the size meant for propane. If this does not achieve satisfactory results, another recommendation is to increase the size of the jets. The pressure of biogas being released through the appliance should be between 75-150 mm of the water column so the flame is stable, compact, and blue (‘Biogas Appliances’). This can be best done with a lotus burner. See Figure 2.

*Figure 2: Example of a Lotus Burner and Flame* (Shutterstock)



*Refrigerator:* Absorption refrigerating machines operating on ammonia and water can be fueled with biogas. The only part which needs to be modified on this appliance is the burner itself. However, one must check that all safety features (e.g. safety pilot) function properly.

*Gas Lamp:* Using biogas as a fuel for light has a very low efficiency (~3%) (‘Biogas Appliances’). This means that the bulb gets very hot and may be a fire hazard. In order to modify the lamp for optimization, there must be a pre-control of biogas supply and air without the mantel. This will result in an elongated flame. Next, the incandescent body and air supply should be adjusted finely. When the flame is too large, the incandescent body will show black spots, therefor the lamp is at its maximum efficiency when the flame is adjusted just smaller than when the black spots appear. This must be done on a biogas specific lamp, and there is no possibility of changing the injector size.

\*One should not discount the possibility of buying an appliance specifically designed for raw biogas input.

**Efficiency of Raw Biogas**

Raw biogas can be used in a variety of ways, as seen above. However, they all have different efficiencies and consumption rates. Estimations of these rates are listed below (‘Biogas Appliances’).

* *Household Burner:* 150-450 L/hr
* *Refrigerator (100 L):* 30-75 L/hr
* *Gas Lamp (60 W Bulb):* 120-160 L/hr

APPENDIX

*Table 3: Recent Studies on the Enhancement of Start-up and Granulation in UASB Reactors*

(adap. Chong et al. 2012)

A screenshot of a cell phone

Description automatically generated

*Table 4: Advantages and Disadvantages of Post-treatment Options* (adap. Chong et al. 2012)

A screenshot of a newspaper

Description automatically generated*Table 5: Advantages and Disadvantages of Post-treatment Options cont.* (adap. Chong et al. 2012)

A screenshot of text

Description automatically generated

*Table 6: Overall Relative Comparison of Reviewed Post-treatment and UASB Options* (adap. Chong et al. 2012)

A screenshot of a social media post

Description automatically generated

REFERENCES

Bhatti, Z. A., Maqbool, F., Malik, A. H., & Mehmood, Q. (2014). UASB reactor startup for the treatment of municipal wastewater followed by advanced oxidation process. Vol. 31 (03), pp. 715–726. <https://doi.org/10.1590/0104-6632.20140313s00002786>

Biogas Appliances. (n.d.). Retrieved from https://energypedia.info/wiki/Biogas\_Appliances.

Burning Blue Flames Gas Focus on Stock Photo (Shutterstock) 1499930861. (n.d.). Retrieved December 10, 2019, from https://www.shutterstock.com/image-photo/burning-blue-flames-gas-focus-on-1499930861

Cavalcanti P.F.F., Van Haandel A., Lettinga G. (2001) Polishing ponds for post-treatment of digested sewage Part 1: flow-through ponds*. Water Sci Technol*, Vol. 44, pp. 237-245.

Chernicharo C.A.L., M.C.P. Nascimento M.C.P. (2001) Feasibility of a pilot-scale UASB/trickling filter system for domestic sewage treatment. *Water Sci Technol*, Vol. 44, pp. 221-228.

Chong, S., Sen, T. K., Kayaalp, A., & Ang, H. M. (2012). The performance enhancements of upflow anaerobic sludge blanket (UASB) reactors for domestic sludge treatment – A State-of-the-art review. *Water Research*, *46*(11), 3434–3470. <https://doi.org/10.1016/J.WATRES.2012.03.066>

Escudie, R., Cresson, R., Delgenes, J.-P., Bernet, N., 2011. Control of start-up and operation of anaerobic biofilm reactors: An overview of 15 years of research. *WATER RESEARCH 45, 1–10.* <https://doi.org/10.1016/j.watres.2010.07.081>

Explaining the Activated Sludge Process. (n.d.). Retrieved December 10, 2019, from <http://www.nesc.wvu.edu/pdf/WW/publications/pipline/PL_SP03.pdf>

Ghangrekar, M.M., Asolekar, S.R., Ranganathan, K.R., Joshi, S.G. (1996). Experience with UASB reactor start-up under different operating conditions. *Water Science and Technology,* Vol.34 (5-6), pp. 421-428.

Hulshoff Pol, L.W., de Castro Lopes, S.I., Lettinga, G., Lens, P.N.L. (2004). Anaerobic sludge granulation. *Water Research,* Vol. 38 (6), pp. 1376-1389.

Khan, A. A., Gaur, R. Z., Tyagi, V. K., Khursheed, A., Lew, B., Mehrotra, I., & Kazmi, A. A. (2011, October). Sustainable options of post treatment of UASB effluent treating sewage: A review. *Resources, Conservation and Recycling*, Vol. 55, pp. 1232–1251. <https://doi.org/10.1016/j.resconrec.2011.05.017>

La Motta, E.J., Silva, E., Bustillos, A., Padro´n, H., Luque, J. (2007). Combined anaerobic/aerobic secondary municipal wastewater treatment: pilot-plant demonstration of the UASB/Aerobic solids contact system. *Journal of Environmental Engineering.* Vol. 133 (4), pp. 397-403.

Lettinga G., Hulshoff Pol L. W. and Zeeman, G. (1993) *Biologische Waterzuivering, Anaërobe Zuivering (biological Wastewater Treatment, Anaerobic Treatment)*. Department of Environmental Technology, Wageningen Agricultural University, The Netherlands.

Machdar I., Harada H., Ohashi A., Sekiguchi Y., Okui H., Ueki K. (1997) A novel and cost-effective sewage treatment system consisting of UASB pre-treatment and aerobic post-treatment units for developing countries. *Water Sci. Technol.*, Vol. 36, pp. 189-197.

Machdar I., Sekiguchi Y., Sumino H., Ohashi A., Harada H. (2000) Combination of a UASB reactor and a curtain type DHS (downflow hanging sponge) reactor as a cost-effective sewage treatment system for developing countries*. Water Sci Technol,* Vol. 42, pp. 83-88.

Moawad A., Mahmoud U.F., El-Khateeb M.A., El-Molla E. (2009). Coupling of sequencing batch reactor and UASB reactor for domestic wastewater treatment. *Desalination*, Vol. 242, pp. 325-335.

Pontes, P.P., Chernicharo, C.A.L., Frade, E.C., Porto, M.T.R. (2003). Performance evaluation of an UASB reactor used for combined treatment of domestic sewage and excess aerobic sludge from a trickling filter. *Water Science and Technology*, Vol. 48 (6), pp. 227-234.

Schmidt, J.E., Ahring, B.K. (1996). Granular sludge formation in upflow anaerobic sludge blanket (UASB) reactors. *Biotechnology and Bioengineering*, Vol. 49 (3), pp. 229-246.

Sousa J.T.,Van Haandel A.C., Guimarães A.A.V. (2001) Post-treatment of anaerobic effluents in constructed wetland systems. *Water Sci Technol*, Vol. 44, pp. 213-219.

Tanigawa S. (2017) Fact Sheet - Biogas: Converting Waste to Energy | White Papers | EESI. Retrieved December 10, 2019, from <https://www.eesi.org/papers/view/fact-sheet-biogasconverting-waste-to-energy>

Tawfik A., Klapwijk B., El-Gohary F., Lettinga G. (2002) Treatment of anaerobically treated domestic wastewater using rotating biological contactor. *Water Sci Technol*, Vol. 45, pp. 371-376.

Torres, P., Foresti, E. (2001). Domestic sewage treatment in a pilot system composed of UASB and SBR reactors. *Water Science and Technology*, Vol. 44 (4), pp. 247-253.

Uemura, S., Takahashi, K., Takaishi, A., Machdar, I., Ohashi, A., Harada, H. (2002). Removal of indigenous coliphages and fecal coliforms by a novel sewage treatment system consisting of UASB and DHS units. *Water Science and Technology,* Vol. 46 (11), pp. 303-309.

Vieira S. (1988) Anaerobic treatment of domestic sewage in Brazil. Research results and full-scale experience. *Proc. 5th. International Symposium on Anaerobic Digestion.* Bologna, Italy. 185-196.

Vlyssides, A., Barampouti, E.M., Mai, S. (2008). Granulation mechanism of a UASB reactor supplemented with iron. *Anaerobe*, Vol. 14 (5), pp. 275-279.

von Sperling M., Freire V.H., Chernicharo C.A.L. (2001) Performance evaluation of a UASB—activated sludge system treating municipal wastewater. *Water Sci Technol*, Vol. 43, pp. 323-328.

von Sperling, M., Chernicharo, C.A.L., Soares, A., Zerbini, A.M. (2003). Evaluation and modelling of helminth eggs removal in baffled and unbaffled ponds treating anaerobic effluent. *Water Science and Technology,* Vol. 48 (2), pp. 113-120.

Upflow Anaerobic Sludge Blanket Reactor (UASB) | SSWM - Find tools for sustainable sanitation and water management! (n.d.). Retrieved December 10, 2019, from https://sswm.info/taxonomy/term/3807/upflow-anaerobic-sludge-blanket-reactor-%28uasb%29

Wastewater Technology Fact Sheet Sequencing Batch Reactors (EPA SBR). (1999).

Wastewater Technology Fact Sheet Trickling Filters (EPA TF). (2000).

Wastewater Treatment (SSWM). (n.d.). Retrieved from http://archive.sswm.info/category/implementation-tools/wastewater-treatment#(Semi-)Centralised Wastewater Treatments.